From 8aab380dded91464d39d1ad1221b75d8a50ed539 Mon Sep 17 00:00:00 2001
From: florian <florian@3c298f89-4303-0410-b956-a3cf2f4a3e73>
Date: Fri, 3 Aug 2007 09:31:47 +0000
Subject: Add some more documentation

git-svn-id: svn://svn.openwrt.org/openwrt/trunk@8330 3c298f89-4303-0410-b956-a3cf2f4a3e73
---
 docs/network.tex | 10 ++++++++++
 1 file changed, 10 insertions(+)

(limited to 'docs/network.tex')

diff --git a/docs/network.tex b/docs/network.tex
index 7d811ba7f..16e5571ae 100644
--- a/docs/network.tex
+++ b/docs/network.tex
@@ -102,3 +102,13 @@ As value it takes a list of ports with these optional suffixes:
 The CPU port defaults to tagged, all other ports to untagged.
 On Broadcom hardware the CPU port is always 5. The other ports may vary with
 different hardware.
+
+For instance, if you wish to have 3 vlans, like one 3-port switch, 1 port in a
+DMZ, and another one as your WAN interface, use the following configuration :
+
+\begin{Verbatim}
+config switch       "eth0"
+    option vlan0    "1 2 3 5*"
+    option vlan1    "0 5"
+    option vlan2    "4 5"
+\end{Verbatim}
-- 
cgit v1.2.3

